With the Beacon 2.0 software running for 2 minutes close it then open the dos software Right when you start the program you are in factory mode so you can change anything for about 2 minutes.

Example on the command line you type in P 0x42 590 ENTER for charge voltage = 59.0v. The IMG is of the software script I used notepad to see contents helped me get the single letter commands. If you do P 0x68 0 it will give you factory access forever.